|  |  |
| --- | --- |
| **PCB Specification card** | |
| **Name** | **DAC END1** |
| **Revision** | **1.0 /** |
| **“multi-circuit-boards.eu” form** | |
| **Article No** | **< optional >** |
| **Layers** | **2** |
| **Estimated dispacth** | **Standard** |
| **Format** | **SinglePieces** |
| Size (x/y) | 125 x 100 mm |
| Quantity | \*\* |
| **Surface finish** | **HASL LeadFree** |
| **Trackwidth- space, annular ring** | **>=300um** |
| **Min. drills** | **>=0.3mm** |
| **Material** | **FR4 1.55 mm** |
| **Cu outer layers (final)** | **35 um** |
| **Solder stop** | **Both sides. Green** |
| **Marking print** | **Top** |
| **E-Test** | **Include** |
| **Cutouts** | **Corresponding to the Gerbers** |